# CPU build options

## Description

The following options are mainly used to change the default behavior of optimizations that target certain CPU features:

- `--cpu-baseline`: minimal set of required CPU features.

    Default value is `min` which provides the minimum CPU features that can safely run on a wide range of platforms within the processor family.

    Note

    During the runtime, NumPy modules will fail to load if any of specified features are not supported by the target CPU (raises Python runtime error).

- `--cpu-dispatch`: dispatched set of additional CPU features.

    Default value is `max -xop -fma4` which enables all CPU features, except for AMD legacy features (in case of X86).

    Note

    During the runtime, NumPy modules will skip any specified features that are not available in the target CPU.

These options are accessible through `distutils` commands `distutils.command.build`, `distutils.command.build_clib` and `distutils.command.build_ext`. They accept a set of CPU features or groups of features that gather several features or special options that perform a series of procedures.

Note

If `build_clib` or `build_ext` are not specified by the user, the arguments of `build` will be used instead, which also holds the default values.

To customize both `build_ext` and `build_clib`:

    cd /path/to/numpy
    python setup.py build --cpu-baseline="avx2 fma3" install --user

To customize only `build_ext`:

    cd /path/to/numpy
    python setup.py build_ext --cpu-baseline="avx2 fma3" install --user

To customize only `build_clib`:

    cd /path/to/numpy
    python setup.py build_clib --cpu-baseline="avx2 fma3" install --user

You can also customize CPU/build options through PIP command:

    pip install --no-use-pep517 --global-option=build \
    --global-option="--cpu-baseline=avx2 fma3" \
    --global-option="--cpu-dispatch=max" ./

## Quick Start

In general, the default settings tend to not impose certain CPU features that may not be available on some older processors. Raising the ceiling of the baseline features will often improve performance and may also reduce binary size.

The following are the most common scenarios that may require changing the default settings:

### I am building NumPy for my local use

And I do not intend to export the build to other users or target a different CPU than what the host has.

Set native for baseline, or manually specify the CPU features in case of option native isn’t supported by your platform:

    python setup.py build --cpu-baseline="native" bdist

Building NumPy with extra CPU features isn’t necessary for this case, since all supported features are already defined within the baseline features:

    python setup.py build --cpu-baseline=native --cpu-dispatch=none bdist

Note

A fatal error will be raised if native isn’t supported by the host platform.

### I do not want to support the old processors of the x86 architecture

Since most of the CPUs nowadays support at least AVX, F16C features, you can use:

    python setup.py build --cpu-baseline="avx f16c" bdist

Note

`--cpu-baseline` force combine all implied features, so there’s no need to add SSE features.

### I’m facing the same case above but with ppc64 architecture

Then raise the ceiling of the baseline features to Power8:

    python setup.py build --cpu-baseline="vsx2" bdist

### Having issues with AVX512 features?

You may have some reservations about including of AVX512 or any other CPU feature and you want to exclude from the dispatched features:

    python setup.py build --cpu-dispatch="max -avx512f -avx512cd \
    -avx512_knl -avx512_knm -avx512_skx -avx512_clx -avx512_cnl -avx512_icl" \
    bdist

## Supported Features

The names of the features can express one feature or a group of features, as shown in the following tables supported depend on the lowest interest:

Note

The following features may not be supported by all compilers, also some compilers may produce different set of implied features when it comes to features like `AVX512`, `AVX2`, and `FMA3`. See Platform differences for more details.

### On x86

Name | Implies | Gathers
--- | --- | ---
`SSE` | `SSE2` |
`SSE2` | `SSE` |
`SSE3` | `SSE` `SSE2` |
`SSSE3` | `SSE` `SSE2` `SSE3` |
`SSE41` | `SSE` `SSE2` `SSE3` `SSSE3` |
`POPCNT` | `SSE` `SSE2` `SSE3` `SSSE3` `SSE41` |
`SSE42` | `SSE` `SSE2` `SSE3` `SSSE3` `SSE41` `POPCNT` |
`AVX` | `SSE` `SSE2` `SSE3` `SSSE3` `SSE41` `POPCNT` `SSE42` |
`XOP` | `SSE` `SSE2` `SSE3` `SSSE3` `SSE41` `POPCNT` `SSE42` `AVX` |
`FMA4` | `SSE` `SSE2` `SSE3` `SSSE3` `SSE41` `POPCNT` `SSE42` `AVX` |
`F16C` | `SSE` `SSE2` `SSE3` `SSSE3` `SSE41` `POPCNT` `SSE42` `AVX` |
`FMA3` | `SSE` `SSE2` `SSE3` `SSSE3` `SSE41` `POPCNT` `SSE42` `AVX` `F16C` |
`AVX2` | `SSE` `SSE2` `SSE3` `SSSE3` `SSE41` `POPCNT` `SSE42` `AVX` `F16C` |
`AVX512F` | `SSE` `SSE2` `SSE3` `SSSE3` `SSE41` `POPCNT` `SSE42` `AVX` `F16C` `FMA3` `AVX2` |
`AVX512CD` | `SSE` `SSE2` `SSE3` `SSSE3` `SSE41` `POPCNT` `SSE42` `AVX` `F16C` `FMA3` `AVX2` `AVX512F` |
`AVX512_KNL` | `SSE` `SSE2` `SSE3` `SSSE3` `SSE41` `POPCNT` `SSE42` `AVX` `F16C` `FMA3` `AVX2` `AVX512F` `AVX512CD` | `AVX512ER` `AVX512PF`
`AVX512_KNM` | `SSE` `SSE2` `SSE3` `SSSE3` `SSE41` `POPCNT` `SSE42` `AVX` `F16C` `FMA3` `AVX2` `AVX512F` `AVX512CD` `AVX512_KNL` | `AVX5124FMAPS` `AVX5124VNNIW` `AVX512VPOPCNTDQ`
`AVX512_SKX` | `SSE` `SSE2` `SSE3` `SSSE3` `SSE41` `POPCNT` `SSE42` `AVX` `F16C` `FMA3` `AVX2` `AVX512F` `AVX512CD` | `AVX512VL` `AVX512BW` `AVX512DQ`
`AVX512_CLX` | `SSE` `SSE2` `SSE3` `SSSE3` `SSE41` `POPCNT` `SSE42` `AVX` `F16C` `FMA3` `AVX2` `AVX512F` `AVX512CD` `AVX512_SKX` | `AVX512VNNI`
`AVX512_CNL` | `SSE` `SSE2` `SSE3` `SSSE3` `SSE41` `POPCNT` `SSE42` `AVX` `F16C` `FMA3` `AVX2` `AVX512F` `AVX512CD` `AVX512_SKX` | `AVX512IFMA` `AVX512VBMI`
`AVX512_ICL` | `SSE` `SSE2` `SSE3` `SSSE3` `SSE41` `POPCNT` `SSE42` `AVX` `F16C` `FMA3` `AVX2` `AVX512F` `AVX512CD` `AVX512_SKX` `AVX512_CLX` `AVX512_CNL` | `AVX512VBMI2` `AVX512BITALG` `AVX512VPOPCNTDQ`
`AVX512_SPR` | `SSE` `SSE2` `SSE3` `SSSE3` `SSE41` `POPCNT` `SSE42` `AVX` `F16C` `FMA3` `AVX2` `AVX512F` `AVX512CD` `AVX512_SKX` `AVX512_CLX` `AVX512_CNL` `AVX512_ICL` | `AVX512FP16`

### On IBM/POWER big-endian

Name | Implies
--- | ---
`VSX` |
`VSX2` | `VSX`
`VSX3` | `VSX` `VSX2`
`VSX4` | `VSX` `VSX2` `VSX3`

### On IBM/POWER little-endian

Name | Implies
--- | ---
`VSX` | `VSX2`
`VSX2` | `VSX`
`VSX3` | `VSX` `VSX2`
`VSX4` | `VSX` `VSX2` `VSX3`

### On ARMv7/A32

Name | Implies
--- | ---
`NEON` |
`NEON_FP16` | `NEON`
`NEON_VFPV4` | `NEON` `NEON_FP16`
`ASIMD` | `NEON` `NEON_FP16` `NEON_VFPV4`
`ASIMDHP` | `NEON` `NEON_FP16` `NEON_VFPV4` `ASIMD`
`ASIMDDP` | `NEON` `NEON_FP16` `NEON_VFPV4` `ASIMD`
`ASIMDFHM` | `NEON` `NEON_FP16` `NEON_VFPV4` `ASIMD` `ASIMDHP`

### On ARMv8/A64

Name | Implies
--- | ---
`NEON` | `NEON_FP16` `NEON_VFPV4` `ASIMD`
`NEON_FP16` | `NEON` `NEON_VFPV4` `ASIMD`
`NEON_VFPV4` | `NEON` `NEON_FP16` `ASIMD`
`ASIMD` | `NEON` `NEON_FP16` `NEON_VFPV4`
`ASIMDHP` | `NEON` `NEON_FP16` `NEON_VFPV4` `ASIMD`
`ASIMDDP` | `NEON` `NEON_FP16` `NEON_VFPV4` `ASIMD`
`ASIMDFHM` | `NEON` `NEON_FP16` `NEON_VFPV4` `ASIMD` `ASIMDHP`

### On IBM/ZSYSTEM(S390X)

Name | Implies
--- | ---
`VX` |
`VXE` | `VX`
`VXE2` | `VX` `VXE`

## Special Options

- `NONE`: enable no features.

- `NATIVE`: Enables all CPU features that supported by the host CPU, this operation is based on the compiler flags (`-march=native`, `-xHost`, `/QxHost`)

- `MIN`: Enables the minimum CPU features that can safely run on a wide range of platforms:

  For Arch | Implies
  --- | ---
  x86 (32-bit mode) | `SSE` `SSE2`
  x86_64 | `SSE` `SSE2` `SSE3`
  IBM/POWER (big-endian mode) | `NONE`
  IBM/POWER (little-endian mode) | `VSX` `VSX2`
  ARMHF | `NONE`
  ARM64 A.K. AARCH64 | `NEON` `NEON_FP16` `NEON_VFPV4` `ASIMD`
  IBM/ZSYSTEM(S390X) | `NONE`

- `MAX`: Enables all supported CPU features by the compiler and platform.

- `Operators-/+`: remove or add features, useful with options `MAX`, `MIN` and `NATIVE`.

## Behaviors

- CPU features and other options are case-insensitive, for example:

      python setup.py build --cpu-dispatch="SSE41 avx2 FMA3"

- The order of the requested optimizations doesn’t matter:

      python setup.py build --cpu-dispatch="SSE41 AVX2 FMA3"
      # equivalent to
      python setup.py build --cpu-dispatch="FMA3 AVX2 SSE41"

- Either commas or spaces or ‘+’ can be used as a separator, for example:

      python setup.py build --cpu-dispatch="avx2 avx512f"
      # or
      python setup.py build --cpu-dispatch=avx2,avx512f
      # or
      python setup.py build --cpu-dispatch="avx2+avx512f"

  all works but arguments should be enclosed in quotes or escaped by backslash if any spaces are used.

- `--cpu-baseline` combines all implied CPU features, for example:

      python setup.py build --cpu-baseline=sse42
      # equivalent to
      python setup.py build --cpu-baseline="sse sse2 sse3 ssse3 sse41 popcnt sse42"

- `--cpu-baseline` will be treated as “native” if compiler native flag `-march=native` or `-xHost` or `/QxHost` is enabled through environment variable CFLAGS:

      export CFLAGS="-march=native"
      python setup.py install --user
      # is equivalent to
      python setup.py build --cpu-baseline=native install --user

- `--cpu-baseline` escapes any specified features that aren’t supported by the target platform or compiler rather than raising fatal errors.

  > Note

  > Since `--cpu-baseline` combines all implied features, the maximum supported of implied features will be enabled rather than escape all of them. For example:

  >     # Requesting `AVX2,FMA3` but the compiler only support **SSE** features
  >     python setup.py build --cpu-baseline="avx2 fma3"
  >     # is equivalent to
  >     python setup.py build --cpu-baseline="sse sse2 sse3 ssse3 sse41 popcnt sse42"

- `--cpu-dispatch` does not combain any of implied CPU features, so you must add them unless you want to disable one or all of them:

      # Only dispatches AVX2 and FMA3
      python setup.py build --cpu-dispatch=avx2,fma3
      # Dispatches AVX and SSE features
      python setup.py build --cpu-baseline=ssse3,sse41,sse42,avx,avx2,fma3

- `--cpu-dispatch` escapes any specified baseline features and also escapes any features not supported by the target platform or compiler without raising fatal errors.

Eventually, you should always check the final report through the build log to verify the enabled features. See Build report for more details.

## Platform differences

Some exceptional conditions force us to link some features together when it come to certain compilers or architectures, resulting in the impossibility of building them separately.

These conditions can be divided into two parts, as follows:

Architectural compatibility

The need to align certain CPU features that are assured to be supported by successive generations of the same architecture, some cases:

- On ppc64le `VSX(ISA 2.06)` and `VSX2(ISA 2.07)` both imply one another since the first generation that supports little-endian mode is Power-8`(ISA 2.07)`

- On AArch64 `NEON NEON_FP16 NEON_VFPV4 ASIMD` implies each other since they are part of the hardware baseline.

For example:

    # On ARMv8/A64, specify NEON is going to enable Advanced SIMD
    # and all predecessor extensions
    python setup.py build --cpu-baseline=neon
    # which equivalent to
    python setup.py build --cpu-baseline="neon neon_fp16 neon_vfpv4 asimd"

Note

Please take a deep look at Supported Features, in order to determine the features that imply one another.

Compilation compatibility

Some compilers don’t provide independent support for all CPU features. For instance Intel’s compiler doesn’t provide separated flags for `AVX2` and `FMA3`, it makes sense since all Intel CPUs that comes with `AVX2` also support `FMA3`, but this approach is incompatible with other x86 CPUs from AMD or VIA.

For example:

    # Specify AVX2 will force enables FMA3 on Intel compilers
    python setup.py build --cpu-baseline=avx2
    # which equivalent to
    python setup.py build --cpu-baseline="avx2 fma3"

The following tables only show the differences imposed by some compilers from the general context that been shown in the Supported Features tables:

Note

Features names with strikeout represent the unsupported CPU features.

### On x86::Intel Compiler

Name | Implies | Gathers
--- | --- | ---
FMA3 | SSE SSE2 SSE3 SSSE3 SSE41 POPCNT SSE42 AVX F16C AVX2 |
AVX2 | SSE SSE2 SSE3 SSSE3 SSE41 POPCNT SSE42 AVX F16C FMA3 |
AVX512F | SSE SSE2 SSE3 SSSE3 SSE41 POPCNT SSE42 AVX F16C FMA3 AVX2 AVX512CD |
XOP | SSE SSE2 SSE3 SSSE3 SSE41 POPCNT SSE42 AVX |
FMA4 | SSE SSE2 SSE3 SSSE3 SSE41 POPCNT SSE42 AVX |
AVX512_SPR | SSE SSE2 SSE3 SSSE3 SSE41 POPCNT SSE42 AVX F16C FMA3 AVX2 AVX512F AVX512CD AVX512_SKX AVX512_CLX AVX512_CNL AVX512_ICL | AVX512FP16

### On x86::Microsoft Visual C/C++

Name | Implies | Gathers
--- | --- | ---
FMA3 | SSE SSE2 SSE3 SSSE3 SSE41 POPCNT SSE42 AVX F16C AVX2 |
AVX2 | SSE SSE2 SSE3 SSSE3 SSE41 POPCNT SSE42 AVX F16C FMA3 |
AVX512F | SSE SSE2 SSE3 SSSE3 SSE41 POPCNT SSE42 AVX F16C FMA3 AVX2 AVX512CD AVX512_SKX |
AVX512CD | SSE SSE2 SSE3 SSSE3 SSE41 POPCNT SSE42 AVX F16C FMA3 AVX2 AVX512F AVX512_SKX |
AVX512_KNL | SSE SSE2 SSE3 SSSE3 SSE41 POPCNT SSE42 AVX F16C FMA3 AVX2 AVX512F AVX512CD | AVX512ER AVX512PF
AVX512_KNM | SSE SSE2 SSE3 SSSE3 SSE41 POPCNT SSE42 AVX F16C FMA3 AVX2 AVX512F AVX512CD AVX512_KNL | AVX5124FMAPS AVX5124VNNIW AVX512VPOPCNTDQ
AVX512_SPR | SSE SSE2 SSE3 SSSE3 SSE41 POPCNT SSE42 AVX F16C FMA3 AVX2 AVX512F AVX512CD AVX512_SKX AVX512_CLX AVX512_CNL AVX512_ICL | AVX512FP16

## Build report

In most cases, the CPU build options do not produce any fatal errors that lead to hanging the build. Most of the errors that may appear in the build log serve as heavy warnings due to the lack of some expected CPU features by the compiler.

So we strongly recommend checking the final report log, to be aware of what kind of CPU features are enabled and what are not.

You can find the final report of CPU optimizations at the end of the build log, and here is how it looks on x86_64/gcc:

    ########### EXT COMPILER OPTIMIZATION ###########
    Platform      :
      Architecture: x64
      Compiler    : gcc

    CPU baseline  :
      Requested   : 'min'
      Enabled     : SSE SSE2 SSE3
      Flags       : -msse -msse2 -msse3
      Extra checks: none

    CPU dispatch  :
      Requested   : 'max -xop -fma4'
      Enabled     : SSSE3 SSE41 POPCNT SSE42 AVX F16C FMA3 AVX2 AVX512F AVX512CD AVX512_KNL AVX512_KNM AVX512_SKX AVX512_CLX AVX512_CNL AVX512_ICL
      Generated   :
                  :
      SSE41       : SSE SSE2 SSE3 SSSE3
      Flags       : -msse -msse2 -msse3 -mssse3 -msse4.1
      Extra checks: none
      Detect      : SSE SSE2 SSE3 SSSE3 SSE41
                  : build/src.linux-x86_64-3.9/numpy/core/src/umath/loops_arithmetic.dispatch.c
                  : numpy/core/src/umath/_umath_tests.dispatch.c
                  :
      SSE42       : SSE SSE2 SSE3 SSSE3 SSE41 POPCNT
      Flags       : -msse -msse2 -msse3 -mssse3 -msse4.1 -mpopcnt -msse4.2
      Extra checks: none
      Detect      : SSE SSE2 SSE3 SSSE3 SSE41 POPCNT SSE42
                  : build/src.linux-x86_64-3.9/numpy/core/src/_simd/_simd.dispatch.c
                  :
      AVX2        : SSE SSE2 SSE3 SSSE3 SSE41 POPCNT SSE42 AVX F16C
      Flags       : -msse -msse2 -msse3 -mssse3 -msse4.1 -mpopcnt -msse4.2 -mavx -mf16c -mavx2
      Extra checks: none
      Detect      : AVX F16C AVX2
                  : build/src.linux-x86_64-3.9/numpy/core/src/umath/loops_arithm_fp.dispatch.c
                  : build/src.linux-x86_64-3.9/numpy/core/src/umath/loops_arithmetic.dispatch.c
                  : numpy/core/src/umath/_umath_tests.dispatch.c
                  :
      (FMA3 AVX2) : SSE SSE2 SSE3 SSSE3 SSE41 POPCNT SSE42 AVX F16C
      Flags       : -msse -msse2 -msse3 -mssse3 -msse4.1 -mpopcnt -msse4.2 -mavx -mf16c -mfma -mavx2
      Extra checks: none
      Detect      : AVX F16C FMA3 AVX2
                  : build/src.linux-x86_64-3.9/numpy/core/src/_simd/_simd.dispatch.c
                  : build/src.linux-x86_64-3.9/numpy/core/src/umath/loops_exponent_log.dispatch.c
                  : build/src.linux-x86_64-3.9/numpy/core/src/umath/loops_trigonometric.dispatch.c
                  :
      AVX512F     : SSE SSE2 SSE3 SSSE3 SSE41 POPCNT SSE42 AVX F16C FMA3 AVX2
      Flags       : -msse -msse2 -msse3 -mssse3 -msse4.1 -mpopcnt -msse4.2 -mavx -mf16c -mfma -mavx2 -mavx512f
      Extra checks: AVX512F_REDUCE
      Detect      : AVX512F
                  : build/src.linux-x86_64-3.9/numpy/core/src/_simd/_simd.dispatch.c
                  : build/src.linux-x86_64-3.9/numpy/core/src/umath/loops_arithm_fp.dispatch.c
                  : build/src.linux-x86_64-3.9/numpy/core/src/umath/loops_arithmetic.dispatch.c
                  : build/src.linux-x86_64-3.9/numpy/core/src/umath/loops_exponent_log.dispatch.c
                  : build/src.linux-x86_64-3.9/numpy/core/src/umath/loops_trigonometric.dispatch.c
                  :
      AVX512_SKX  : SSE SSE2 SSE3 SSSE3 SSE41 POPCNT SSE42 AVX F16C FMA3 AVX2 AVX512F AVX512CD
      Flags       : -msse -msse2 -msse3 -mssse3 -msse4.1 -mpopcnt -msse4.2 -mavx -mf16c -mfma -mavx2 -mavx512f -mavx512cd -mavx512vl -mavx512bw -mavx512dq
      Extra checks: AVX512BW_MASK AVX512DQ_MASK
      Detect      : AVX512_SKX
                  : build/src.linux-x86_64-3.9/numpy/core/src/_simd/_simd.dispatch.c
                  : build/src.linux-x86_64-3.9/numpy/core/src/umath/loops_arithmetic.dispatch.c
                  : build/src.linux-x86_64-3.9/numpy/core/src/umath/loops_exponent_log.dispatch.c
    CCompilerOpt.cache_flush[804] : write cache to path -> /home/seiko/work/repos/numpy/build/temp.linux-x86_64-3.9/ccompiler_opt_cache_ext.py

    ########### CLIB COMPILER OPTIMIZATION ###########
    Platform      :
      Architecture: x64
      Compiler    : gcc

    CPU baseline  :
      Requested   : 'min'
      Enabled     : SSE SSE2 SSE3
      Flags       : -msse -msse2 -msse3
      Extra checks: none

    CPU dispatch  :
      Requested   : 'max -xop -fma4'
      Enabled     : SSSE3 SSE41 POPCNT SSE42 AVX F16C FMA3 AVX2 AVX512F AVX512CD AVX512_KNL AVX512_KNM AVX512_SKX AVX512_CLX AVX512_CNL AVX512_ICL
      Generated   : none

There is a separate report for each of `build_ext` and `build_clib` that includes several sections, and each section has several values, representing the following:

Platform:

- Architecture: The architecture name of target CPU. It should be one of `x86`, `x64`, `ppc64`, `ppc64le`, `armhf`, `aarch64`, `s390x` or `unknown`.

- Compiler: The compiler name. It should be one of gcc, clang, msvc, icc, iccw or unix-like.

CPU baseline:

- Requested: The specific features and options to `--cpu-baseline` as-is.

- Enabled: The final set of enabled CPU features.

- Flags: The compiler flags that were used to all NumPy C/C++ sources during the compilation except for temporary sources that have been used for generating the binary objects of dispatched features.

- Extra checks: list of internal checks that activate certain functionality or intrinsics related to the enabled features, useful for debugging when it comes to developing SIMD kernels.

CPU dispatch:

- Requested: The specific features and options to `--cpu-dispatch` as-is.

- Enabled: The final set of enabled CPU features.

- Generated: At the beginning of the next row of this property, the features for which optimizations have been generated are shown in the form of several sections with similar properties explained as follows:

  - One or multiple dispatched feature: The implied CPU features.

  - Flags: The compiler flags that been used for these features.

  - Extra checks: Similar to the baseline but for these dispatched features.

  - Detect: Set of CPU features that need be detected in runtime in order to execute the generated optimizations.

  - The lines that come after the above property and end with a ‘:’ on a separate line, represent the paths of c/c++ sources that define the generated optimizations.

## Runtime dispatch

Importing NumPy triggers a scan of the available CPU features from the set of dispatchable features. This can be further restricted by setting the environment variable `NPY_DISABLE_CPU_FEATURES` to a comma-, tab-, or space-separated list of features to disable. This will raise an error if parsing fails or if the feature was not enabled. For instance, on `x86_64` this will disable `AVX2` and `FMA3`:

    NPY_DISABLE_CPU_FEATURES="AVX2,FMA3"

If the feature is not available, a warning will be emitted.