# numpy.fft.fft

fft.fft(a, n=None, axis=-1, norm=None)

  Compute the one-dimensional discrete Fourier Transform.

  This function computes the one-dimensional n-point discrete Fourier Transform (DFT) with the efficient Fast Fourier Transform (FFT) algorithm [CT].

  Parameters:
    a array_like

      Input array, can be complex.

    n int, optional

      Length of the transformed axis of the output. If n is smaller than the length of the input, the input is cropped. If it is larger, the input is padded with zeros. If n is not given, the length of the input along the axis specified by axis is used.

    axis int, optional

      Axis over which to compute the FFT. If not given, the last axis is used.

    norm{“backward”, “ortho”, “forward”}, optional

      New in version 1.10.0.

      Normalization mode (see `numpy.fft`). Default is “backward”. Indicates which direction of the forward/backward pair of transforms is scaled and with what normalization factor.

      New in version 1.20.0: The “backward”, “forward” values were added.

  Returns:
    out complex ndarray

      The truncated or zero-padded input, transformed along the axis indicated by axis, or the last one if axis is not specified.

  Raises:
    IndexError

      If axis is not a valid axis of a.

  See also

  `numpy.fft`

    for definition of the DFT and conventions used.

  `ifft`

    The inverse of `fft`.

  `fft2`

    The two-dimensional FFT.

  `fftn`

    The n-dimensional FFT.

  `rfftn`

    The n-dimensional FFT of real input.

  `fftfreq`

    Frequency bins for given FFT parameters.

  Notes

  FFT (Fast Fourier Transform) refers to a way the discrete Fourier Transform (DFT) can be calculated efficiently, by using symmetries in the calculated terms. The symmetry is highest when n is a power of 2, and the transform is therefore most efficient for these sizes.

  The DFT is defined, with the conventions used in this implementation, in the documentation for the `numpy.fft` module.

  References

  [CT]

  Cooley, James W., and John W. Tukey, 1965, “An algorithm for the machine calculation of complex Fourier series,” Math. Comput. 19: 297-301.

  Examples

      >>> np.fft.fft(np.exp(2j * np.pi * np.arange(8) / 8))
      array([-2.33486982e-16+1.14423775e-17j,  8.00000000e+00-1.25557246e-15j,
              2.33486982e-16+2.33486982e-16j,  0.00000000e+00+1.22464680e-16j,
             -1.14423775e-17+2.33486982e-16j,  0.00000000e+00+5.20784380e-16j,
              1.14423775e-17+1.14423775e-17j,  0.00000000e+00+1.22464680e-16j])

  In this example, real input has an FFT which is Hermitian, i.e., symmetric in the real part and anti-symmetric in the imaginary part, as described in the `numpy.fft` documentation:

      >>> import matplotlib.pyplot as plt
      >>> t = np.arange(256)
      >>> sp = np.fft.fft(np.sin(t))
      >>> freq = np.fft.fftfreq(t.shape[-1])
      >>> plt.plot(freq, sp.real, freq, sp.imag)
      [<matplotlib.lines.Line2D object at 0x...>, <matplotlib.lines.Line2D object at 0x...>]
      >>> plt.show()